

**Gigaset A540 Analogue Cordless Phone**







**Basic Instructions**

***How to make a call?***

***For external calls:***

**Enter 0** and **the number** on the keypad, then press the **Talk**  Key to connect.

To end the call, press the **End**  key.

***For internal calls:***

Enter the **3-digit internal number** on the keypad, then press the **Talk**  key to connect.

To end the call, press the **End** key.

***How to redial a number you called?***

Press the **Talk**  key once, list will display of dialled calls, scroll down with arrow up and down key**, to highlight,** then press the **Talk**  key to dial the number.

***How to answer an incoming call?***


Press the **Talk**  Key to accept the call

If ***auto answer*** is enabled, pick up the phone from the cradle and the call is answered.

**Basic Instructions**

***How to transfer an incoming call to another phone?***

Whilst on a call-in progress, press the **R**  key, then **you hear system tone**, **dial the number** you wish to transfer to, the **other party answers**, then press the **End ** key to transfer.



***For Technical Support, please call Nu Teck Communications: 02 9647 3333***